GR, OL, KN 27.2.2023

**Open points for 1st release of APC WEB UI**

# Alarming

Two tables for alarming

* Application Log (log for all application related entries, for IHT only) max 3000 entries
* Business log (all station and system events for the user) max 10.000 entries

Export of both logs must be possible. To be send to iht.

Access to alarm list via  button (without no of alarms) Symbol is blue when no message. Red when message, blinking when alarm needs acknowledgement.

When Alarm is on and need ack, by pressing the button, all alarms are acknowledged and alarm list will be show.

Alarm list shows latest alarm at the top. When new alarm arrive, it will be shown at the top.

# CALIB

* Should be moved to Manual Mode
* In Manual Calibration, the height should be part of the CALIB button

# Process mode (idle)

* Three Sliders are grey, and value is zero (maybe showing required nozzle and sensor (splash protector)

# Process mode (active)

* Three Sliders are grey, and value is the value of the current process step (scaling is min and max scaling!
* By pressing the field of the slider (nozzle) a window appears with the slider bigger and active (only when preheating and cutting is active).
* Reload preheat time should have rotating indicator and time in the button

# Menu

* Process mode get a home symbol (house) and PROCESS
* Manual mode get person symbol and MANUAL
* Cutting Data get a table  or symbol and CUTTING DATA

# Setting

Indicate active station!

# IHT colors are:

|  |  |  |
| --- | --- | --- |
| **RGB** | 0, 97, 166 | 243,146,0 |
| **CMYK** | 100,50,1,10 | 0,50,100,0 |